SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( M41-2128
comment (  

Parameterezeshez felhasznalt forrasok:

	1. Az M41 sorozatu dizelmozdony szerkezete, mukodese es kezelese
	2. Vontatasi mechanika es energetika
	3. Vasuti vontatojarmuvek uzemeltetesi zsebkonyve
	4. Vasuti jarmuvek minosito meresei
	5. Vasuti fekberendezesek szerkezete, uzeme es a karbantartas iranyelvei
	6. Vasuti dizeljarmu vezetok zsebkonyve
	7. MSTS technikai leirasok + program binaris valtozata...
	8. GPS + stopperes meresi adatok

Az irodalmi hivatkozasok formaja: [mu sorszama/oldalszam]

)

	Type ( Engine )
        WagonShape ( M41-2128.s )
        Size ( 3.303m 4.393m 15.47m )
        Mass ( 66t ) comment ( [1/9] )       
	WheelRadius ( 0.520m ) 
	InertiaTensor ( Box ( 3.303m 4.393m 15.47m ) )
	comment	( Coupling )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.27 0.47 1.8 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*66t )
	DerailBufferForce ( 330kN )
comment(	NumWheels (	8 ) ) comment ( Futokerek nincs a mozdonyon, tapaadast javitani kell. )
	Friction (
		706.6N/m/s		0		0.7mph		7.354N/m/s		1.84
		5.1N/rad/s		1		-1rad/s		0			1
	)
	comment ( Sajnos nem lehetett konstanst hozzaadni ezert hasznalom ezt a kozelitest )
	comment ( Fme(irodalmi)=2000+10*v(km/h)+0.35*v^2(km/h) [2/37, 3/336])
	comment ( Fme(MSTS)=230*v(m/s) )
	comment ( 60km/h felett meresekkel igazoltan viszonylag kis hibaval mukodik )

	AntiSlip () comment ( Perdulesvedelem van [6/86] )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	
	MaxBrakeForce( 130kN ) comment ( Osszfektuskoero 930kN [2/147] )
#	MaxHandbrakeForce()
#	NumberOfHandbrakeLeverSteps()

	EmergencyBrakeResMaxPressure( 55.1 ) comment ( Ilyen nincs valosagban az M62-esen, 3.8bar = 55.1psi )
#	TrainPipeLeakRate()
#	AuxilaryLeakRate()
	TripleValveRatio( 2.92 ) comment ( Dokumentacio szerint: 3.8bar[fekheng]/{5bar[fovez-toltott]-3.4[fovez-min]} [1/101],[4/284] )
	MaxReleaseRate( 11 ) comment  ( 5 s fekhenger uritesi ido 55psi/5s = 11psi/s csak mozdonyra /becsult/ )
	MaxApplicationRate( 18 ) comment ( 3 s fekhenger toltesi ido 55psi/3s = 18psi/s csak mozdonyra /becsult/ )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 ) comment ( 3.8bar = 55.1psi )
		comment ( Irodalmi adat min. 4 bar [6/175] )

	BrakeDistributorFullServicePressure( 50.75 ) comment ( 3.5bar = 50.75psi [1/101])
	BrakeDistributorMaxAuxilaryResPressure( 72.5 )
		comment ( Valosagban a keszletlegtartaly a folegtartaly vezetekrol kap
			  taplalast, igy 10bar lenne a nyomas, de a muszerek csak igy
			  mutatnak helyes erteket. 5bar = 72.5 psi [1/100] )
	BrakeDistributorEmergencyResPressure( 55.1 ) comment ( Ilyen valosagban nincs, 3.8bar = 55.1psi [1/101])
	BrakeDistributorReleaseRate( 11 ) comment ( u.a. mint MaxReleaseRate )
	BrakeDistributorApplicationRate( 18 ) comment ( u.a. mint MaxApplicationRate )
	BrakeDistributorTrainPipeControlRatio( 2.375 ) comment ( u.a. mint TripleValveRatio )
	BrakeDistributorNormalFullReleasePressure( 72.5 ) comment ( 5bar = 72.5 psi [4/284]) 

	IntakePoint ( -3.33 0.4 FuelDiesel )
	IntakePoint ( 3.33 0.4 FuelDiesel )

		Lights ( 34
 Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( aaffe095 )
     Position ( 1.02 1.82 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( aaffe095 )
     Position ( -1.02 1.82 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( aaffe095 )
     Position ( 1.02 1.82 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( aaffe095 )
     Position ( -1.02 1.82 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
 Light (
  Comment ( Fénysugár reflektor )
   Type  ( 1 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 3.5 4 )
     Transition ( 0 )
     Radius ( 300.0 )
     Angle ( 15.0 )
     )
    )
   )
 Light (
  Comment ( Fénysugár tompított )
   Type  ( 1 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 3.5 4 )
     Transition ( 0 )
     Radius ( 120.0 )
     Angle ( 20.0 )
     )
    )
   )
  Light (
  Comment ( A végi bal belső tompított 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi bal belső tompított 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( A végi jobb belső tompított 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi jobb belső tompított 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 7.5 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light	(
  comment( A végi csúcsfényszóró tompított )
  Type	( 0 )
  Conditions	(
  Headlight ( 2 )
  Unit ( 2 )
  )
  FadeIn  ( 0.5 )
  FadeOut ( 0.5 )
  Cycle	( 0 )
  States ( 1
  State	(
  Duration ( 0.0 )
  LightColour ( 80ffc080 )
  Position ( 0.0 3.63 7.3 )
  Azimuth ( 0.0 -5.0 5.0 )
  Transition ( 0 )
  Radius ( 0.5 )
     )
    )
   )
 Light (
  Comment ( A végi csúcsfényszóró reflektor )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 3.7 7.35 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 1.0 )
     )
    )
   )
  Light (
  Comment ( A végi bal belső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 7.5 )
     Azimuth ( -0.9 -0.9 -0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi bal belső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 7.5 )
     Azimuth ( -0.9 -0.9 -0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( A végi jobb belső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 7.5 )
     Azimuth ( 0.9 0.9 0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi jobb belső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 7.5 )
     Azimuth ( 0.9 0.9 0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( A végi bal külső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -1.04 1.81 7.5 )
     Azimuth ( 0.9 0.9 0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi bal külső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -1.04 1.81 7.5 )
     Azimuth ( 0.9 0.9 0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( A végi jobb külső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 1.04 1.81 7.5 )
     Azimuth ( -0.9 -0.9 -0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( A végi jobb külső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 1.04 1.81 7.5 )
     Azimuth ( -0.9 -0.9 -0.9 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( B végi bal belső tompított 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi bal belső tompított 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( B végi jobb belső tompított 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi jobb belső tompított 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 -7.5 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light	(
  comment( B végi csúcsfényszóró tompított )
  Type	( 0 )
  Conditions	(
  Headlight ( 2 )
  Unit ( 5 )
  )
  FadeIn  ( 0.5 )
  FadeOut ( 0.5 )
  Cycle	( 0 )
  States ( 1
  State	(
  Duration ( 0.0 )
  LightColour ( 80ffc080 )
  Position ( 0.0 3.63 -7.3 )
  Azimuth ( 180.0 -175.0 175.0 )
  Transition ( 0 )
  Radius ( 0.5 )
     )
    )
   )
 Light (
  Comment ( B végi csúcsfényszóró reflektor )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 3.7 -7.35 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 1.0 )
     )
    )
   )
  Light (
  Comment ( B végi bal belső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 -7.5 )
     Azimuth ( -179.1 -179.1 -179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi bal belső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.74 1.81 -7.5 )
     Azimuth ( -179.1 -179.1 -179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( B végi jobb belső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 -7.5 )
     Azimuth ( 179.1 179.1 179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi jobb belső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.74 1.81 -7.5 )
     Azimuth ( 179.1 179.1 179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( B végi bal külső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -1.04 1.81 -7.5 )
     Azimuth ( 179.1 179.1 179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi bal külső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -1.04 1.81 -7.5 )
     Azimuth ( 179.1 179.1 179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
  Light (
  Comment ( B végi jobb külső reflektor 1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 1.04 1.81 -7.5 )
     Azimuth ( -179.1 -179.1 -179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 Light (
  Comment ( B végi jobb külső reflektor 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 1.04 1.81 -7.5 )
     Azimuth ( -179.1 -179.1 -179.1 )
     Transition ( 0 )
     Radius ( 0.35 )
     )
    )
   )
 )


    	Sound (	m41eng_V2b.sms" )
	)

Engine ( M41-2128
	Effects
		(
		DieselSpecialEffects
			(
				comment
				(
					the format of these little blocks is as follow:

					offset.x offset.y offset.z
					normal.x normal.y normal.z
					width in metres

					defining the offset from the shape pivot point
					where steam / smoke should appear, the direction
					it should go and the width of the nozzle
				)

				Exhaust1
				(
					0.0 4.4 -0.7
					0 1 0
					0.3
				)
			)
        	)
        
	Wagon ( M41-2128 )
	Type ( Diesel )
	MaxPower ( 912kW ) 
		comment ( Ugyan 1336kW a beepitett motorteljesitmeny, de
			  a villamos futes 250kW[6/67] es segeduzem 112kW [6/67]
			  miatt legfeljebb kb. 1140kW [3/340] veheto igenybe.
			  0.8 hajtomu hatasfokot figyelembe veve [1/9, 3/340] ez 912 kW.
			  Erdemes megjegyezni tovabba, hogy a Voith L720 hajtomu
			  behajto meretezett teljesitmenye is csak 1044kW [1/26] 
			  Erdekes tovabba az irodalmi adatok 100kW-tal torteno
			  elterese 1140<=>1044. A tapasztalati ertekek a 912kW
			  koruli kerekkeruleti teljesitmenyt igazoltak.)
	MaxForce ( 197kN ) comment ( [1/9], [3/337] )
	MaxContinuousForce ( 137kN ) comment ( [3/355-357], [6/89] )
	MaxVelocity ( 100kmh ) comment ( [1/7] )
	WheelRadius ( 0.520m )
	Sanding ( 1e9mph )
	
	NumWheels ( 4 ) comment ( Realisabbak igy a tapadasi viszonyok! )
	MaxTemperature ( 90 ) comment ( 90C [6/88] )
	MaxOilPressure ( 101.5 ) comment ( 7bar=101.5psi [6/88] )

 	CabView ( "m41_v2.cvf" )
	HeadOut (  1.7 3.0 5.4 )

	MaxDieselLevel ( 3000l ) comment ( [1/9] )
	DieselUsedPerHourAtMaxPower ( 223l ) comment ( 210g/kWh [1/8] )
	DieselUsedPerHourAtIdle ( 18.5l ) comment ( [3/342] )

	AirBrakesAirCompressorPowerRating( 1.54 )
		comment ( VV450/150 legsurito 2620l/min [1/8]= 1.54 ft3/s )
	AirBrakesMainMinResAirPressure( 81.2 ) comment ( 5.6bar = 81.2psi [1/37])
	AirBrakesMainMaxAirPressure( 145 ) comment ( 10bar = 145psi [1/37])
	AirBrakesMainResVolume( 47.7 )	comment ( 3x450l = 47.7ft3 [1/37])
	AirBrakesAirCompressorWattage( 19000 ) comment ( V63 adat )
	AirBrakesCompressorRestartPressure( 128 ) comment ( 8.8bar = 128 psi [1/37])
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 11.3 ) 
		comment ( Passz. Levego igeny fontban. 8in x 90-120mm loket x 4 fekhenger [1/102])
	AirBrakesIsCompressorElectricOrMechanical( 1 ) comment ( villamos legsurito )

	EngineBrakesControllerDirectControlExponent( 1 )

comment(	TrainBrakesControllerMinPressureReduction( 6 ) )

	EngineBrakesControllerHasProportionalBrake( 1 ) comment ( Uzemi fekezeskor a mozdony is fekez )
	EngineBrakesProportionalBrakeLag( 1 ) comment ( Alaphelyzetben nincs utanfekezes )

	comment ( Adatok szemelyvonati P fekuzemre vonatkoznak! )
	EngineBrakesControllerMaxApplicationRate( 6.7 ) comment ( kb 3s -> 6.7 psi/s [4/284])
	TrainBrakesControllerMaxApplicationRate( 4 ) comment ( kb 5s -> 4 psi/s [5/19])
	EngineBrakesControllerMaxReleaseRate( 4 ) comment ( kb 5s -> 4 psi/s [4/284])
	TrainBrakesControllerMaxReleaseRate( 1.3 ) comment ( kb 15s -> 1.3 psi/s [5/20])
	EngineBrakesControllerEmergencyApplicationRate( 25 ) comment ( 5bar->0bar kb 2-3s -> kb 25psi/s [4/285])
	TrainBrakesControllerEmergencyApplicationRate( 25 )

	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 ) comment ( fovezetek ny. 5bar=72.5 psi )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 ) comment ( gyorsfek azonnal oldhato! )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )

	EngineBrakesControllerFullServicePressureDrop( 23.2 ) comment ( 5bar-3.4bar=1.6bar=23.2psi [4/284])
	TrainBrakesControllerFullServicePressureDrop( 23.2 )
	comment ( VAGY: BrakeCylinderPressureForMaxBrakeBrakeForce(55.1)/TripleValveRatio(2.375)=23.2 ) 

	comment ( Magyar rendszer ket vezetekes: fovezetek + folegtartaly vezetek [1/100])
	BrakesEngineBrakeType( "Air_twin_pipe"  )
	BrakesTrainBrakeType( "Air_twin_pipe" )
         	
	comment ( Ket fekkar, Onmukodo fekberendezes: D12, nem onmukodo: Zbr 3,7 )
        BrakesEngineControllers( "Independent, Train" )
        
	MaxDieselLevel ( 2500l )
	DieselUsedPerHourAtMaxPower ( 100l )
	DieselUsedPerHourAtIdle ( 30l )

	DieselSmokeEffectInitialMagnitude( 0.5 )
	DieselSmokeEffectMaxMagnitude( 1.0 )
	DieselSmokeEffectInitialSmokeRate( 0.5 )
	DieselSmokeEffectMaxSmokeRate( 1.0 )	
	
	DieselEngineIdleRPM( 650 )
	DieselEngineMaxRPM( 1515 )
	DieselEngineSpeedOfMaxTractiveEffort( 18kmh ) comment ( [3/355-357] )
	DieselEngineMaxRPMChangeRate( 70 )
	
	DoesHornTriggerBell( 0 )

	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 1 )
    		)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 61 )
		MonitoringDeviceResetLevel( 0.1 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed( 5 )
		MonitoringDeviceDoesSuppressionReset( 0 )
		MonitoringDeviceTriggerOnOverspeed( 75 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
	EngineVariables( 2500l )
	
	comment ( Dizelmotor fokozatok kiosztasa [1/48], [6/75] )		
	comment (  650 1/min 0.00, 114kW  0.00)
	comment (  720 1/min 0.08, 168kW  0.04)
	comment (  810 1/min 0.18, 250kW  0.11)
	comment (  891 1/min 0.28, 338kW  0.18)
	comment (  963 1/min 0.36, 450kW  0.27)
	comment ( 1034 1/min 0.44, 576kW  0.38)
	comment ( 1096 1/min 0.52, 705kW  0.48)
	comment ( 1157 1/min 0.59, 847kW  0.60)
	comment ( 1212 1/min 0.65, 978kW  0.71)
	comment ( 1268 1/min 0.71, 1107kW 0.81)
	comment ( 1322 1/min 0.78, 1186kW 0.88)
	comment ( 1370 1/min 0.83, 1228kW 0.91)
	comment ( 1419 1/min 0.89, 1265kW 0.94)
	comment ( 1461 1/min 0.94, 1296kW 0.97)
	comment ( 1500 1/min 0.98, 1324kW 0.99)
	comment ( 1515 1/min 1.00, 1337kw 1.00)   
        EngineControllers (
            Throttle ( 0 1 0.125 0
                NumNotches ( 16
                    Notch ( 0       0 Dummy )
                    Notch ( 0.02    0 Dummy )
                    Notch ( 0.10    0 Dummy )
                    Notch ( 0.18    0 Dummy )
                    Notch ( 0.27    0 Dummy )
                    Notch ( 0.38    0 Dummy )
                    Notch ( 0.47    0 Dummy )
                    Notch ( 0.60    0 Dummy )
		    	  Notch ( 0.71    0 Dummy )
                    Notch ( 0.81    0 Dummy )
                    Notch ( 0.88    0 Dummy )
                    Notch ( 0.91    0 Dummy )
                    Notch ( 0.94    0 Dummy )
                    Notch ( 0.97    0 Dummy )
                    Notch ( 0.99    0 Dummy )
                    Notch ( 1.00    0 Dummy )
                )
            )
            Brake_Engine ( 0 1 0.1 0 
                NumNotches ( 1
                    Notch ( 0       1 Dummy )                    
                )
            )
	    comment ( M62-esen tesztelt es a konnyu kezelhetosege miatt nalam
			bevalt fekkontroller. Az Acela HHP-8 fekezoszelep vezerlesenek
			modositott valtozata. )
            Brake_Train ( 0 1 0.1 0.70
                NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerHoldStart )
                    Notch ( 0.2  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            BailOffButton( 0 1 0 )
        )
        
    	Sound (	"m41cab_V2b.sms" )
    	Name ( "M41 2128" )
        Description (
	"Developer: Virtual Modelling Works.\n"+
	"http://www.train-sim.hu\n\n"+
	"Manufacturer: GANZ-MAVAG\n\n"+
	"Mnfr. serie: DHM-7\n\n"+
	"Mnfr. year: 1973-1984\n\n"+
	"Total number built for MAV: 114\n\n"+
	"Traction: Diesel-Hydraulic\n\n"+
	"Diesel engine: 12 Pa4-185 12 Cylinders with turbocharger\n\n"+
	"Cont. power: 1325 kW\n\n"+
	"Max. speed: 100 km/h\n\n"+
	"Wheel diameter:1040 mm\n\n"+
	"Height: 4230 mm\n\n"+
	"Width: 3092 mm\n\n"+
	"Total lenght: 15500 mm\n\n"+
	"Weight: 66 tons\n\n"+
	"Wheel arrangement: B'B'"

    	)
    	EngineOperatingProcedures (
    	"To move forward\n"+
	"1.	Press the W key to move the Reverser to Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"4.	Press the D key to move the throttle from Idle to Notch 1.\n"+
	"5.	Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the dynamic brakes\n"+
	"1.	Press the A key to move the throttle to the Idle position.\n"+
	"2.	Wait for 10 seconds, then press the . (PERIOD) key to advance the Dynamic Brake handle from Off to the Setup position. After allowing a few seconds for braking circuit setup, press the . (PERIOD) key again to set the desired level of dynamic braking (Levels 1 - 8).\n\n"+
	"To release the dynamic brakes\n"+
	"1. Press the D key to move the throttle towards Idle.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
    	) 
)

